HU-FRIEDY PEDO & PERMANENTNÍ KORUNKY NEREZOVÉ KORUNKY NA MOLÁRY – PRIMÁRNÍ A PERMANENTNÍ 
Návod k použití:
 Nerezové korunky Hu-Friedy jsou určeny k úplnému krytí, silnějšímu a provizornímu ošetření primárních molárů a k uspokojení potřeby dlouhodobého provizorního krytí stálých molárů. 
Aby se minimalizovalo konturování a ořezávání, jsou tyto nerezové primární a trvalé korunky na moláry předem krimpované, předem zvlněné a předem olemované. 
Výběr a příprava korunky 
1. Vyberte správnou velikost korunky. Změřte meziodistální rozměr zubu v ústech pacienta. Poté změřte korunky ze sady, abyste určili odpovídající velikost. 
2. Jakmile je určena správná velikost, otestujte, zda přesně sedí v ústech. Zkontrolujte okluzi  mezi protilehlými a sousedními zuby.
3. Pomocí sondy zkontrolujte případné otevřené okraje mezi preparací a korunkou. V případě potřeby korunku upravte, abyste dosáhli lepšího okrajového usazení. 
4. Pokud dochází k nadměrnému zblednutí gingivální tkáně při usazení korunky, bude nutné korunku zastřihnout. Nesmazatelným perem nebo voskovou tužkou označte korunku podle obrysu gingivy. Pomocí nůžek na korunky zastřihněte 1 mm pod značkou. Snažte se řezat plynulým pohybem, abyste se vyhnuli vzniku ostrých okrajů, které by mohly dráždit tkáň pacienta. Pokud se vytvoří ostrá místa, použijte k odstranění brusný kámen a vyleštěte je gumovým kotoučem. K úpravě tvaru a krimpování korunky v oříznutých okrajích použijte konturovací kleště. Proveďte další zkušební usazení, abyste zajistili přesnost, správný kontakt a okluzi. 
5. Proveďte další zkušební usazení, abyste zajistili přesnost, správný kontakt a zkontrolovali okluzi. 
6. Při kontrole okluze si pečlivě všímejte všech rozdílů ve vztahu maxila/mandibula. Pokud je korunka plně usazena a brání správnému skusu, může být nutná další redukce preparace. Zub mírně dále redukujte a znovu zkuste korunku nasadit, abyste ověřili správný skus. 
Usazení korunky 
1. Izolujte preparovaný zub umístěním kofferdamu nebo pomocí vatových tamponů. 
2. Preparaci omyjte a důkladně osušte. 
3. Smíchejte cement a naplňte vybranou korunku podle pokynů výrobce cementu. 
4. Usaďte korunku. Doporučení: u dolní čelisti začněte na lingvální ploše a tlačte směrem k bukální ploše; u maxilárních korunek začněte na bukální ploše a tlačte směrem k lingvální ploše. To pomůže vytlačit zbytkový cement. Během konečného usazení nepoužívejte nadměrnou sílu. 
5. Během počátečního usazení korunky ověřte správné zarovnání kontrolou vztahu se sousedními zuby a protilehlými zuby. Po potvrzení správného zarovnání poučte pacienta, aby skousl do gázy nebo okluzální skusové tyčinky; Tím zajistíte, že korunka bude plně usazena do správného skusu. Pokud používáte pomůcku k usazení korunky během cementování, buďte opatrní, abyste dosáhli správného skusu. Nepoužívejte nadměrnou sílu, abyste korunku neusadili pod úroveň správného skusu. 
6. Dodržujte pokyny výrobce cementu a odstraňte přebytečný cement v určeném čase. Odstranění cementu lze provést pomocí exploreru, scaleru nebo exkavátoru. K odstranění cementu z interproximálních ploch a subgingiválních oblastí použijte dentální nit. 
Korunky z nerezové oceli Hu-Friedy jsou vyrobeny ze slitiny nerezové oceli, která obsahuje elementární nikl a chrom. Malé procento populace je na tyto kovy alergické. Pokud se objeví alergická reakce, požádejte pacienta, aby se poradil s lékařem. 
Tento produkt je určen pouze pro zubní lékaře. 
Tento produkt je jednorázový; opakované použití je zakázáno. 
Mezi potenciální rizika v případě opětovného použití produktu patří: 
• Zavlečení mikrobů do těla v důsledku opětovného použití předmětu, který mohl být kontaminován během jeho prvního použití, což může vést k následnému zhoršení zdravotního stavu pacienta 
• Poranění měkkých tkání od ostrých hran, pokud byla korunka dříve ořezána 
Uchovávejte produkt při pokojové teplotě a mimo dosah přímého slunečního záření.




















HU-FRIEDY PEDO & PERMANENT CROWNS STAINLESS STEEL PRIMARY AND PERMANENT MOLAR CROWNS 
Instructions for Use 
Hu-Friedy’s Stainless Steel Crowns are intended to provide full coverage, stronger, provisional treatment for primary molars and fill the need for long term provisional coverage on permanent molars. To help minimize contouring and trimming, these stainless steel primary and permanent molar crowns are precrimped, prebelled and prefestooned. 
Crown Selection and Preparation 
1. Select the proper crown size. Measure the mesio-distal dimension of the tooth in the patient’s mouth. Next, measure the crowns in the kit to determine the corresponding size. 
2. Once the appropriate size has been identified, test for accurate fit in the mouth. Note the occlusal relationship between the opposing teeth and the relationship to the adjacent dentition. 
3. Using an explorer, probe for any open margins between the preparation and the crown. If necessary, reshape the crown to achieve a better marginal fit. 
4. If there is excessive blanching of the gingival tissue when the crown is seated, the crown will need to be trimmed. Using an indelible pen or wax pencil, mark the crown following the contour of the gingiva. Use crown scissors to trim 1 mm below the mark. Try to cut in a smooth motion to avoid producing sharp metal burs that might irritate the patient’s tissue. If sharp areas are produced, use a heatless stone to remove the burs and polish with a rubber wheel. Use contouring pliers to reshape and crimp the crown at the trimmed margins. Complete another test fit to ensure accuracy, proper contacts and occlusion. 
5. Complete another try-in fit to ensure accuracy, proper contact and check the occlusion.
 6. When checking the occlusion, carefully notice any differences in the maxillary/mandibular relationship. If the crown is fully seated and the crown prevents proper occlusion, further reduction of the preparation may be necessary. Slightly reduce the tooth further and re-try the crown once again to confirm proper occlusion. 
Seating the Crown 
1. Isolate the prepared tooth by placing rubber dam or by using cotton rolls. 
2. Wash and thoroughly dry the preparation. 
3. Mix the cement and fill the selected crown, following cement manufacturer’s instructions. 
4. Seat the crown. Recommendation: for mandibular crowns start at the lingual surface, pressing across to the buccal surface; for maxillary crowns start at the buccal surface, pressing across to the lingual. This will assist in the residual cement being squeezed out. Do not use excessive force during final seating. 
5. During the initial seating of the crown, verify proper alignment by checking the relationship with adjacent teeth and opposing teeth. When proper alignment is confirmed, instruct the patient to bite on gauze or an occlusal bite stick; this will ensure the crown is fully seated into the proper occlusion. If using a device to assist in crown seating during cementation, please use care to obtain proper occlusion. Do not use excessive force in order to avoid seating the crown below the level of proper occlusion. 
6. Following individual cement manufacturer’s instructions, remove the excess cement at the allocated time. Cement removal can be done with an explorer, scaler, or excavator. Use dental floss to remove cement from the interproximal surfaces and subgingival areas. 
Hu-Friedy Stainless Steel Crowns are made with a stainless steel alloy that contains elemental nickel and chromium. A small percentage of the population is known to be allergic to these metals. If an allergic reaction occurs, direct the patient to consult a physician. 
This product is intended for use only by dental professionals. 
This product is single use (disposable); reuse is prohibited. 
Potential risks if the product was reused include: 
• Introduction of microbes into the body due to reuse of item which may have been contaminated during its first use, which can result in subsequent health deterioration of patient • Soft tissue injury from any rough edges if the crown was previously trimmed Keep product at room temperature and out of direct sunlight. 
To reorder Hu-Friedy Pedo and Permanent Crowns, call 1-800-Hu-Friedy. N3342/1219 1-800-Hu-Friedy Hu-Friedy.com Manufactured for: Hu-Friedy Mfg. Co., LLC: 3232 N. Rockwell St. | Chicago, IL 60
